{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":9,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"merged":[[0,0,0,10],[1,0,1,10],[2,9,2,10],[15,8,15,10],[16,8,16,10]],"flags":["formulas_cached_only"]}
["泰州市姜城水务有限责任公司每周出厂水水质公示"]
["    为保证城乡居民饮用水安全，接受社会监督，现将我公司供水水质指标予以公示。此次水质公示采样日期为2025年12月15日至2025年12月21日，采样监测结果显示，我公司出厂水水质达到国家生活饮用水卫生标准要求。"]
["采样地点","二水厂送水泵房","水样类型","出厂水","采样环境","正常环境","检验方式","化学检验","消毒方式","次氯酸钠"]
["序号","项目","单位","限值","12月15日        检验值","12月16日        检验值","12月17日        检验值","12月18日        检验值","12月19日        检验值","12月20日        检验值","12月21日        检验值"]
[1,"总大肠菌群","MPN/100mL","不应检出","未检出","未检出","未检出","未检出","未检出","未检出","未检出"]
[2,"大肠埃希氏菌","MPN/100mL","不应检出","未检出","未检出","未检出","未检出","未检出","未检出","未检出"]
[3,"菌落总数","CFU/mL","≤100","未检出","未检出",1,"未检出","未检出","未检出","未检出"]
[4,"色度                        (铂钴色度单位)","度","≤15","<5","<5","<5","<5","<5","<5","<5"]
[5,"浑浊度                  (散射浑浊度单位)","NTU","≤1",0.07,0.08,0.07,0.06,0.08,0.09,0.13]
[6,"臭和味","级",0,0,0,0,0,0,0,0]
[7,"肉眼可见物","--","无","无","无","无","无","无","无","无"]
[8,"pH","--","≥6.5且≤8.5",7.59,7.57,7.56,7.48,7.61,7.59,{"v":7.6,"d":"7.60"}]
[9,"高锰酸盐指数","mg/L","≤3",1.08,1.08,1.04,0.92,{"v":1,"d":"1.00"},0.89,{"v":1,"d":"1.00"}]
[10,"游离氯","mg/L","≥0.3",0.7,0.8,0.7,0.7,0.7,0.7,0.6]
[]
[{"$nulls":8},"泰州市姜城水务有限责任公司"]
[{"$nulls":8},"水质检测中心"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}