{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":9,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"merged":[[0,0,0,10],[1,0,1,10],[2,9,2,10],[15,8,15,10],[16,8,16,10]],"flags":["formulas_cached_only"]}
["泰州市姜城水务有限责任公司每周出厂水水质公示"]
["    为保证城乡居民饮用水安全，接受社会监督，现将我公司供水水质指标予以公示。此次水质公示采样日期为2026年1月26日至2026年2月1日，采样监测结果显示，我公司出厂水水质达到国家生活饮用水卫生标准要求。"]
["采样地点","二水厂送水泵房","水样类型","出厂水","采样环境","正常环境","检验方式","化学检验","消毒方式","次氯酸钠"]
["序号","项目","单位","限值","1月26日        检验值","1月27日        检验值","1月28日        检验值","1月29日        检验值","1月30日        检验值","1月31日        检验值","2月1日        检验值"]
[1,"总大肠菌群","MPN/100mL","不应检出","未检出","未检出","未检出","未检出","未检出","未检出","未检出"]
[2,"大肠埃希氏菌","MPN/100mL","不应检出","未检出","未检出","未检出","未检出","未检出","未检出","未检出"]
[3,"菌落总数","CFU/mL","≤100","未检出","未检出","未检出",1,2,"未检出",1]
[4,"色度                        (铂钴色度单位)","度","≤15","<5","<5","<5","<5","<5","<5","<5"]
[5,"浑浊度                  (散射浑浊度单位)","NTU","≤1",0.09,0.09,0.09,0.09,{"v":0.1,"d":"0.10"},0.08,0.09]
[6,"臭和味","级",0,0,0,0,0,0,0,0]
[7,"肉眼可见物","--","无","无","无","无","无","无","无","无"]
[8,"pH","--","≥6.5且≤8.5",7.63,7.58,7.64,7.62,7.62,7.62,7.66]
[9,"高锰酸盐指数","mg/L","≤3",1.02,0.99,1.09,1.15,1.02,1.02,1.02]
[10,"游离氯","mg/L","≥0.3",0.6,0.6,0.6,0.6,0.6,0.7,0.7]
[]
[{"$nulls":8},"泰州市姜城水务有限责任公司"]
[{"$nulls":8},"水质检测中心"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}